CREATE VPN SERVER IN WINDOWS

1.View Network Connections
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2.Create Username for better security purpose to be only for vpn
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3- Create DHCP RANGE THAT DOESN’T MATCH WITH THE ROUTER TO AVOID IP CONFLICT like
192.168.1.230 to 192.168.1.235
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Then click Allow access






Allow Windows Firewall to allow external connections : 
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Turn On Private & Public 
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Port Forward VPN Port to The Server IP / Hostname
XXXX.dyndns.info or Ip Address
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Allow/Enable in Security tab PPTP if exists in the router  : 
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New Incomming Connection has been created to allow the Vpn users to  connect 
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CONNECT TO VPN SERVER
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You add the username and the password that has been created in the vpn server, once saved you can connect to the VPN and disconnect whenever needed.
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